
FLOW AND VOLUME OUTPUT SUMMARY
==============================

Initial Water Volume Within Domain (m3)....................=            0.00
Cumulative Gross Rainfall Volume Entering Domain (m3)......=    190430800.00
Cumulative Interception Volume Within Domain (m3)..........=            0.00
Cumulative Net Rainfall Volume Entering Domain (m3)........=    190430800.00
Cumulative Rainfall Excess (Rain-Intercept-Infilt) (m3)....=      7587008.00
Flow Volume Entering Domain from External Sources (m3).....=            0.00
  Volume Entering the Overland Plane (m3).....= 0.000000
  Volume Entering the Channel Network (m3)....= 0.000000
Cumulative Volume Entering Domain, V_in (m3)...............=    190430800.00
Volume leaving the Watershed, V_out (m3)...................=    185771615.50
Percentage of V_out to V_in (%)............................=           97.55
Volume leaving the Watershed via Overland Flow (m3)........=            0.00
Volume leaving the Watershed via Channel Flow (m3).........=      2927823.50
Percentage of Overland/Channel Outflow to V_in (%).........=            1.54
Final Surface Volume, V_final (m3).........................=      2735559.94
  Final Surface Volume, Overland (m3).........= 956227.937500
  Final Surface Volume, Channels (m3).........= 1779332.000000
Percentage of V_final to V_in (%)..........................=            1.44
Percentage of Overland/Channel Outflow to V_in-V_final (%).=            1.56
Volume Infiltrated Overland, V_inf (m3)....................=    182843792.00
Percentage of (V_inf + V_ctl) to V_in (%)..................=           96.02

Percent Mass Balance Error (%).............................=            1.01

MINIMUM AND MAXIMUM VALUES FOR SELECT HYDROLOGIC/HYDRAULIC PROCESSES
=====================================================================

Outlet: 1 (Row 134, Col 185)
Peak Channel Discharge (m3/s)..............................=           32.35
Time to Peak (hours).......................................=           28.24

Min. Rainfall Intensity (mm/hr)............................=           -0.00
Max. Rainfall Intensity (mm/hr)............................=          103.75

Min. Infiltration Depth (mm)...............................=            0.00
Max. Infiltration Depth (mm)...............................=          285.89


Transmission loss was not simulated

Min. Overland Depth (m)....................................=           0.000
Max. Overland Depth (m)....................................=           0.831

Min. Channel Depth (m).....................................=           0.000
Max. Channel Depth (m).....................................=           4.547




Runtime Performance Summary
~~~~~~~~~~~~~~~~~~~~~~~~~~~

TREX model run successfully completed! 
Program stopped at simulation hour:     72.0011

TREX Run Time:     14.95 minutes
