NOTE 15301:  Began computing simulation run "Bankfull" at time 18Jul2019, 11:47:58.
NOTE 20364:  Found no parameter problems in meteorologic model "Bankfull".
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-1 NFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-1 NFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-2 NFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-2 NFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-1 SFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-1 SFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-2 SFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-2 SFS" because storage is zero.
WARNING 41074:  Length for reach "Reach-1" is very short and may cause numeric instabilities.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-3 NFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-3 NFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-3 SFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-3 SFS" because storage is zero.
NOTE 40049:  Found no parameter problems in basin model "Cheyenne at Evans Compromise".
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1 SFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2 SFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3 SFS" is less than the simulation time interval.
WARNING 40012:  Could not compute observed flow for element "Junction-2".
NOTE 41054:  Routing parameters for reach "Reach-1": Delta t (sec) 14.6  Delta x (m) 30.25
WARNING 40012:  Could not compute observed flow for element "Junction-2".
WARNING 40013:  Could not compute residual flow for element "Junction-2".
NOTE 15302:  Finished computing simulation run "Bankfull" at time 18Jul2019, 11:47:58.
