NOTE 15301:  Began computing simulation run "Comb_HMS_6-hr 10^2-yr" at time 24Jun2021, 10:24:13.
NOTE 20364:  Found no parameter problems in meteorologic model "6-hr 10^2-yr".
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-1".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-1" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-2".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-2" because storage is zero.
WARNING 41074:  Length for reach "Reach-1" is very short and may cause numeric instabilities.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-3".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-3" because storage is zero.
NOTE 40049:  Found no parameter problems in basin model "Cheyenne_60cm".
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2" is less than the simulation time interval.
NOTE 41089:  Routing parameters based on index flow 20.0 m3/s for reach "Reach-1": Delta t (sec) 31.0  Delta x (m) 60.5000
NOTE 41102:  Index flow 20.0 (m3/s) for reach "Reach-1" translates to an index celerity of 1.94 (m/s).
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3" is less than the simulation time interval.
WARNING 40012:  Could not compute observed flow for element "Junction-2".
NOTE 42413:  Unit hydrograph volume for subbasin "Subbasin-1" is 1.0000 mm.
NOTE 42413:  Unit hydrograph volume for subbasin "Subbasin-2" is 1.0000 mm.
NOTE 42413:  Unit hydrograph volume for subbasin "Subbasin-3" is 1.0000 mm.
NOTE 41079:  Routing incremental distance for reach "Reach-1" is based on specified index flow 20 m3/s.  Calculated index flow from minimum (0.0) and maximum (5.3) inflow is 3 m3/s.
WARNING 41084:  Applying the diffusivity criteria using index flow 3 m3/s at reach "Reach-1" would have increased spatial steps from 1 to 2.
WARNING 40012:  Could not compute observed flow for element "Junction-2".
WARNING 40013:  Could not compute residual flow for element "Junction-2".
WARNING 40012:  Could not compute observed flow for element "Junction-2".
WARNING 40026:  Could not compute cumulative observed flow for element "Junction-2".
NOTE 15302:  Finished computing simulation run "Comb_HMS_6-hr 10^2-yr" at time 24Jun2021, 10:24:13.
