NOTE 15301:  Began computing simulation run "Uncal_Var_ClarkUH_10^7yr_2hr" at time 23Aug2022, 19:58:36.
NOTE 20364:  Found no parameter problems in meteorologic model "2-hr 10^7-yr".
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-2".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-2" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-1".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-1" because storage is zero.
WARNING 41074:  Length for reach "Reach-1" is very short and may cause numeric instabilities.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-3".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-3" because storage is zero.
NOTE 40049:  Found no parameter problems in basin model "CheyCr_Uncal_Var_ClarkUH".
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1" is less than the simulation time interval.
NOTE 41089:  Routing parameters based on index flow 20.0 m3/s for reach "Reach-1": Delta t (sec) 31.0  Delta x (m) 60.5000
NOTE 41102:  Index flow 20.0 (m3/s) for reach "Reach-1" translates to an index celerity of 1.94 (m/s).
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3" is less than the simulation time interval.
WARNING 40012:  Could not compute Observed Flow for element "Junction-2".
NOTE 45913:  Clark Tc=1.13 hr, R=5.25 hr for period ending at 1 January 2000, 00:15 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.40 hr, R=5.25 hr for period ending at 1 January 2000, 00:15 for subbasin "Subbasin-1".
NOTE 45913:  Clark Tc=0.27 hr, R=5.25 hr for period ending at 1 January 2000, 00:15 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=0.97 hr, R=4.49 hr for period ending at 1 January 2000, 00:30 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.26 hr, R=4.72 hr for period ending at 1 January 2000, 00:30 for subbasin "Subbasin-1".
WARNING 45918:  Clark Tc=0.23 hr increased to the allowed minimum Tc=0.25 hr at subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=0.25 hr, R=4.42 hr for period ending at 1 January 2000, 00:30 for subbasin "Subbasin-3".
WARNING 12465:  Requested interpolation value 1,872.1899 is above the last value 1,824 in table "Sub2".
WARNING 12465:  Requested interpolation value 1,872.1899 is above the last value 1,824 in table "Sub2".
NOTE 45913:  Clark Tc=1.13 hr, R=5.25 hr for period ending at 1 January 2000, 00:45 for subbasin "Subbasin-2".
WARNING 12465:  Requested interpolation value 3,120.0432 is above the last value 3,063 in table "Sub1".
WARNING 12465:  Requested interpolation value 3,120.0432 is above the last value 3,063 in table "Sub1".
NOTE 45913:  Clark Tc=1.40 hr, R=5.25 hr for period ending at 1 January 2000, 00:45 for subbasin "Subbasin-1".
WARNING 12465:  Requested interpolation value 1,719.1142 is above the last value 1,674 in table "Sub3".
WARNING 12465:  Requested interpolation value 1,719.1142 is above the last value 1,674 in table "Sub3".
NOTE 45913:  Clark Tc=0.27 hr, R=5.25 hr for period ending at 1 January 2000, 00:45 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=0.56 hr, R=2.61 hr for period ending at 1 January 2000, 01:00 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=0.71 hr, R=2.64 hr for period ending at 1 January 2000, 01:00 for subbasin "Subbasin-1".
WARNING 45918:  Clark Tc=0.14 hr increased to the allowed minimum Tc=0.25 hr at subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=0.25 hr, R=2.65 hr for period ending at 1 January 2000, 01:00 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=0.93 hr, R=4.33 hr for period ending at 1 January 2000, 01:15 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.16 hr, R=4.35 hr for period ending at 1 January 2000, 01:15 for subbasin "Subbasin-1".
WARNING 45918:  Clark Tc=0.23 hr increased to the allowed minimum Tc=0.25 hr at subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=0.25 hr, R=4.41 hr for period ending at 1 January 2000, 01:15 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=1.08 hr, R=5.02 hr for period ending at 1 January 2000, 01:30 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.36 hr, R=5.08 hr for period ending at 1 January 2000, 01:30 for subbasin "Subbasin-1".
NOTE 45913:  Clark Tc=0.26 hr, R=5.13 hr for period ending at 1 January 2000, 01:30 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=1.13 hr, R=5.25 hr for period ending at 1 January 2000, 01:45 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.40 hr, R=5.25 hr for period ending at 1 January 2000, 01:45 for subbasin "Subbasin-1".
NOTE 45913:  Clark Tc=0.27 hr, R=5.25 hr for period ending at 1 January 2000, 01:45 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=1.13 hr, R=5.25 hr for period ending at 1 January 2000, 02:00 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.40 hr, R=5.25 hr for period ending at 1 January 2000, 02:00 for subbasin "Subbasin-1".
NOTE 45913:  Clark Tc=0.27 hr, R=5.25 hr for period ending at 1 January 2000, 02:00 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=1.13 hr, R=5.25 hr for period ending at 1 January 2000, 02:15 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.40 hr, R=5.25 hr for period ending at 1 January 2000, 02:15 for subbasin "Subbasin-1".
NOTE 45913:  Clark Tc=0.27 hr, R=5.25 hr for period ending at 1 January 2000, 02:15 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=1.13 hr, R=5.25 hr for period ending at 1 January 2000, 02:30 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.40 hr, R=5.25 hr for period ending at 1 January 2000, 02:30 for subbasin "Subbasin-1".
NOTE 45913:  Clark Tc=0.27 hr, R=5.25 hr for period ending at 1 January 2000, 02:30 for subbasin "Subbasin-3".
NOTE 45913:  Clark Tc=1.13 hr, R=5.25 hr for period ending at 1 January 2000, 02:45 for subbasin "Subbasin-2".
NOTE 45913:  Clark Tc=1.40 hr, R=5.25 hr for period ending at 1 January 2000, 02:45 for subbasin "Subbasin-1".
NOTE 45913:  Clark Tc=0.27 hr, R=5.25 hr for period ending at 1 January 2000, 02:45 for subbasin "Subbasin-3".
NOTE 41079:  Routing incremental distance for reach "Reach-1" is based on specified index flow 20 m3/s.  Calculated index flow from minimum (0.0) and maximum (229.7) inflow is 115 m3/s.
WARNING 40012:  Could not compute Observed Flow for element "Junction-2".
WARNING 40013:  Could not compute Residual Flow for element "Junction-2".
WARNING 40012:  Could not compute Observed Flow for element "Junction-2".
WARNING 40026:  Could not compute cumulative observed flow for element "Junction-2".
NOTE 15302:  Finished computing simulation run "Uncal_Var_ClarkUH_10^7yr_2hr" at time 23Aug2022, 19:58:38.
NOTE 15312:  The total runtime for this simulation is 00:02.
