NOTE 15351:  Began computing optimization trial "RMSE_Sep2013_GISCurves" at time 24Sep2019, 10:56:06.
NOTE 20364:  Found no parameter problems in meteorologic model "Sep2013".
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-1 NFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-1 NFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-2 NFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-2 NFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-1 SFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-1 SFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-2 SFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-2 SFS" because storage is zero.
WARNING 41074:  Length for reach "Reach-1" is very short and may cause numeric instabilities.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-3 NFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-3 NFS" because storage is zero.
WARNING 45220:  No plant uptake method selected for subbasin "Subbasin-3 SFS".  There will be no transpiration for loss method: Soil Moisture Accounting.
WARNING 42014:  No percolation or outflow will be computed for layer 2 in subbasin "Subbasin-3 SFS" because storage is zero.
NOTE 40049:  Found no parameter problems in basin model "Cheyenne at Evans_GISCurves".
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1 SFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2 SFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3 SFS" is less than the simulation time interval.
WARNING 10783:  There are no unlocked parameters to optimize.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-1 SFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-2 SFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3 NFS" is less than the simulation time interval.
WARNING 42012:  Storage coefficient for layer 2 in subbasin "Subbasin-3 SFS" is less than the simulation time interval.
NOTE 41054:  Routing parameters for reach "Reach-1": Delta t (sec) 15.5  Delta x (m) 30.25
NOTE 15352:  Finished computing optimization trial "RMSE_Sep2013_GISCurves" at time 24Sep2019, 10:56:07.
