<?xml version="1.0" encoding="UTF-8"?>
<RunResults>
  <RunName>Sep2013_AORC_Uncalib</RunName>
  <Description>Basin: Cheyenne_60cm , Meteorology: Sep2013_AORC , Control: Sep2013</Description>
  <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
  <StartTime>08Sep2013, 02:00</StartTime>
  <EndTime>18Sep2013, 01:00</EndTime>
  <BasinElement name="Subbasin-1" type="Subbasin">
    <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
    <SubbasinArea area="29.77" units="KM2" />
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="29.77" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Incremental Precip" displayString="Precipitation" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-INC//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Precip" displayString="Cumulative Precipitation" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-CUM//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Reference ET" displayString="Reference Evapotranspiration" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-REFERENCE//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Excess" displayString="Canopy Overflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/EXCESS-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Potential ET" displayString="Potential Evapotranspiration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-POTENTIAL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy ET" displayString="Canopy Evapotranspiration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Storage" displayString="Canopy Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/STORAGE-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Infiltration" displayString="Soil Infiltration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/INFILTRATION//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Storage" displayString="Soil Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/STORAGE-SOIL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Percolation" displayString="Soil Percolation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/PERC-SOIL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Saturation Fraction" displayString="Saturation Fraction" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/SATURATION FRACTION//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Storage" displayString="Groundwater 1 Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/STORAGE-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Release" displayString="Groundwater 1 Lateral Flow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/OUTFLOW-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Percolation" displayString="Groundwater 1 Percolation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/PERC-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Excess" displayString="Excess Precipitation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-EXCESS//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Excess" displayString="Cumulative Excess Precipitation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-EXCESS-CUM//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Loss" displayString="Precipitation Loss" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-LOSS//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Loss" displayString="Cumulative Precipitation Loss" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-LOSS-CUM//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Direct Runoff" displayString="Direct Runoff" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-DIRECT//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Baseflow" displayString="Baseflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-BASE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Aquifer Recharge" displayString="Aquifer Recharge" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-1/AQUIFER RECHARGE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="0.0000000" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="0.0000000" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="4.4832251" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="13Sep2013, 00:45" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="1270697.6312820" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="42.6838304" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="1.4756987" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum" displayString="Minimum Direct Flow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum Time" displayString="Time of Minimum Direct Flow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Direct Flow Maximum" displayString="Maximum Direct Flow" value="2.3328092" units="M3/S" />
      <StatisticMeasure type="Direct Flow Maximum Time" displayString="Time of Maximum Direct Flow" value="13Sep2013, 00:30" />
      <StatisticMeasure type="Direct Flow Volume" displayString="Direct Flow Volume" value="323649.2531388" units="M3" />
      <StatisticMeasure type="Direct Flow Depth" displayString="Direct Flow Depth" value="10.8716578" units="MM" />
      <StatisticMeasure type="Direct Flow Average" displayString="Direct Flow Average" value="0.3757683" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum" displayString="Minimum Baseflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum Time" displayString="Time of Minimum Baseflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Baseflow Maximum" displayString="Maximum Baseflow" value="3.0344637" units="M3/S" />
      <StatisticMeasure type="Baseflow Maximum Time" displayString="Time of Maximum Baseflow" value="13Sep2013, 18:15" />
      <StatisticMeasure type="Baseflow Volume" displayString="Baseflow Volume" value="947048.3781432" units="M3" />
      <StatisticMeasure type="Baseflow Depth" displayString="Baseflow Depth" value="31.8121726" units="MM" />
      <StatisticMeasure type="Baseflow Average" displayString="Baseflow Average" value="1.0999304" units="M3/S" />
      <StatisticMeasure type="Precipitation Maximum" displayString="Maximum Precipitation" value="5.5000000" units="MM" />
      <StatisticMeasure type="Precipitation Maximum Time" displayString="Time of Maximum Precipitation" value="12Sep2013, 17:00" />
      <StatisticMeasure type="Precipitation Total" displayString="Precipitation Total" value="234.6500011" units="MM" />
      <StatisticMeasure type="Precipitation Volume" displayString="Precipitation Volume" value="6985530.5317845" units="M3" />
      <StatisticMeasure type="Loss Maximum" displayString="Maximum Loss" value="5.2260417" units="MM" />
      <StatisticMeasure type="Loss Maximum Time" displayString="Time of Maximum Loss" value="12Sep2013, 17:00" />
      <StatisticMeasure type="Loss Total" displayString="Loss Total" value="223.7783343" units="MM" />
      <StatisticMeasure type="Loss Volume" displayString="Loss Volume" value="6661881.0135286" units="M3" />
      <StatisticMeasure type="Excess Maximum" displayString="Maximum Excess" value="0.2739583" units="MM" />
      <StatisticMeasure type="Excess Maximum Time" displayString="Time of Maximum Excess" value="12Sep2013, 17:00" />
      <StatisticMeasure type="Excess Total" displayString="Excess Total" value="10.8716667" units="MM" />
      <StatisticMeasure type="Excess Volume" displayString="Excess Volume" value="323649.5182559" units="M3" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Subbasin-2" type="Subbasin">
    <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
    <SubbasinArea area="26.54" units="KM2" />
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="26.54" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Incremental Precip" displayString="Precipitation" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-INC//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Precip" displayString="Cumulative Precipitation" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-CUM//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Reference ET" displayString="Reference Evapotranspiration" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-2/ET-REFERENCE//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Excess" displayString="Canopy Overflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/EXCESS-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Potential ET" displayString="Potential Evapotranspiration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/ET-POTENTIAL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy ET" displayString="Canopy Evapotranspiration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/ET-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Storage" displayString="Canopy Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/STORAGE-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Infiltration" displayString="Soil Infiltration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/INFILTRATION//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Storage" displayString="Soil Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/STORAGE-SOIL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Percolation" displayString="Soil Percolation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/PERC-SOIL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Saturation Fraction" displayString="Saturation Fraction" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/SATURATION FRACTION//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Storage" displayString="Groundwater 1 Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/STORAGE-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Release" displayString="Groundwater 1 Lateral Flow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/OUTFLOW-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Percolation" displayString="Groundwater 1 Percolation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/PERC-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Excess" displayString="Excess Precipitation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-EXCESS//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Excess" displayString="Cumulative Excess Precipitation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-EXCESS-CUM//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Loss" displayString="Precipitation Loss" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-LOSS//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Loss" displayString="Cumulative Precipitation Loss" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-LOSS-CUM//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Direct Runoff" displayString="Direct Runoff" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW-DIRECT//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Baseflow" displayString="Baseflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW-BASE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Aquifer Recharge" displayString="Aquifer Recharge" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-2/AQUIFER RECHARGE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="0.0000000" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="0.0000000" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="23.9885252" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="2282780.8396223" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="86.0128425" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="2.6505323" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum" displayString="Minimum Direct Flow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum Time" displayString="Time of Minimum Direct Flow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Direct Flow Maximum" displayString="Maximum Direct Flow" value="20.9505229" units="M3/S" />
      <StatisticMeasure type="Direct Flow Maximum Time" displayString="Time of Maximum Direct Flow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Direct Flow Volume" displayString="Direct Flow Volume" value="1233042.9662084" units="M3" />
      <StatisticMeasure type="Direct Flow Depth" displayString="Direct Flow Depth" value="46.4597953" units="MM" />
      <StatisticMeasure type="Direct Flow Average" displayString="Direct Flow Average" value="1.4316068" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum" displayString="Minimum Baseflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum Time" displayString="Time of Minimum Baseflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Baseflow Maximum" displayString="Maximum Baseflow" value="3.7684787" units="M3/S" />
      <StatisticMeasure type="Baseflow Maximum Time" displayString="Time of Maximum Baseflow" value="14Sep2013, 00:30" />
      <StatisticMeasure type="Baseflow Volume" displayString="Baseflow Volume" value="1049737.8734140" units="M3" />
      <StatisticMeasure type="Baseflow Depth" displayString="Baseflow Depth" value="39.5530472" units="MM" />
      <StatisticMeasure type="Baseflow Average" displayString="Baseflow Average" value="1.2189255" units="M3/S" />
      <StatisticMeasure type="Precipitation Maximum" displayString="Maximum Precipitation" value="7.9167500" units="MM" />
      <StatisticMeasure type="Precipitation Maximum Time" displayString="Time of Maximum Precipitation" value="12Sep2013, 17:00" />
      <StatisticMeasure type="Precipitation Total" displayString="Precipitation Total" value="297.7980003" units="MM" />
      <StatisticMeasure type="Precipitation Volume" displayString="Precipitation Volume" value="7903558.9277229" units="M3" />
      <StatisticMeasure type="Loss Maximum" displayString="Maximum Loss" value="3.8551387" units="MM" />
      <StatisticMeasure type="Loss Maximum Time" displayString="Time of Maximum Loss" value="12Sep2013, 17:00" />
      <StatisticMeasure type="Loss Total" displayString="Loss Total" value="251.3382050" units="MM" />
      <StatisticMeasure type="Loss Volume" displayString="Loss Volume" value="6670515.9615145" units="M3" />
      <StatisticMeasure type="Excess Maximum" displayString="Maximum Excess" value="4.9310023" units="MM" />
      <StatisticMeasure type="Excess Maximum Time" displayString="Time of Maximum Excess" value="12Sep2013, 17:45" />
      <StatisticMeasure type="Excess Total" displayString="Excess Total" value="46.4597953" units="MM" />
      <StatisticMeasure type="Excess Volume" displayString="Excess Volume" value="1233042.9662084" units="M3" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Junction-1" type="Junction">
    <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="56.31" units="KM2" />
    <FlowLink upstreamName="Subbasin-1" />
    <FlowLink upstreamName="Subbasin-2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Combined Inflow" displayString="Combined Inflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-COMBINE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="28.4085499" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="3553478.4709043" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="63.1056379" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="4.1262310" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="28.4085499" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="3553478.4709043" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="63.1056379" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="4.1262310" units="M3/S" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Reach-1" type="Reach">
    <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="56.31" units="KM2" />
    <FlowLink upstreamName="Junction-1" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Combined Inflow" displayString="Combined Inflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW-COMBINE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Flow Velocity" displayString="Flow Velocity" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW-VELOCITY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="28.4085499" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="3553478.4709043" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="63.1056379" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="4.1262310" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="28.4037312" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="3553458.4445897" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="63.1052823" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="4.1262079" units="M3/S" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Subbasin-3" type="Subbasin">
    <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
    <SubbasinArea area="0.05" units="KM2" />
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="0.05" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Incremental Precip" displayString="Precipitation" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-INC//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Precip" displayString="Cumulative Precipitation" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-CUM//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Reference ET" displayString="Reference Evapotranspiration" />
        <DssFileName>Sep2013_AORC.dss</DssFileName>
        <DssPathname>//Subbasin-3/ET-REFERENCE//15MIN/MET:Sep2013_AORC/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Excess" displayString="Canopy Overflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/EXCESS-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Potential ET" displayString="Potential Evapotranspiration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/ET-POTENTIAL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy ET" displayString="Canopy Evapotranspiration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/ET-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Storage" displayString="Canopy Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/STORAGE-CANOPY//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Infiltration" displayString="Soil Infiltration" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/INFILTRATION//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Storage" displayString="Soil Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/STORAGE-SOIL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Percolation" displayString="Soil Percolation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/PERC-SOIL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Saturation Fraction" displayString="Saturation Fraction" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/SATURATION FRACTION//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Storage" displayString="Groundwater 1 Storage" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/STORAGE-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Release" displayString="Groundwater 1 Lateral Flow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/OUTFLOW-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Percolation" displayString="Groundwater 1 Percolation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/PERC-GW-1//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Excess" displayString="Excess Precipitation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-EXCESS//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Excess" displayString="Cumulative Excess Precipitation" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-EXCESS-CUM//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Loss" displayString="Precipitation Loss" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-LOSS//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Loss" displayString="Cumulative Precipitation Loss" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-LOSS-CUM//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Direct Runoff" displayString="Direct Runoff" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW-DIRECT//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Baseflow" displayString="Baseflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW-BASE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Aquifer Recharge" displayString="Aquifer Recharge" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Subbasin-3/AQUIFER RECHARGE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="0.0000000" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="0.0000000" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="0.0468955" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="12Sep2013, 21:15" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="4276.5263777" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="85.5305276" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="0.0049664" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum" displayString="Minimum Direct Flow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum Time" displayString="Time of Minimum Direct Flow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Direct Flow Maximum" displayString="Maximum Direct Flow" value="0.0441277" units="M3/S" />
      <StatisticMeasure type="Direct Flow Maximum Time" displayString="Time of Maximum Direct Flow" value="12Sep2013, 21:15" />
      <StatisticMeasure type="Direct Flow Volume" displayString="Direct Flow Volume" value="2000.4702290" units="M3" />
      <StatisticMeasure type="Direct Flow Depth" displayString="Direct Flow Depth" value="40.0094046" units="MM" />
      <StatisticMeasure type="Direct Flow Average" displayString="Direct Flow Average" value="0.0023226" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum" displayString="Minimum Baseflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum Time" displayString="Time of Minimum Baseflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Baseflow Maximum" displayString="Maximum Baseflow" value="0.0071676" units="M3/S" />
      <StatisticMeasure type="Baseflow Maximum Time" displayString="Time of Maximum Baseflow" value="14Sep2013, 08:15" />
      <StatisticMeasure type="Baseflow Volume" displayString="Baseflow Volume" value="2276.0561487" units="M3" />
      <StatisticMeasure type="Baseflow Depth" displayString="Baseflow Depth" value="45.5211230" units="MM" />
      <StatisticMeasure type="Baseflow Average" displayString="Baseflow Average" value="0.0026438" units="M3/S" />
      <StatisticMeasure type="Precipitation Maximum" displayString="Maximum Precipitation" value="9.0249996" units="MM" />
      <StatisticMeasure type="Precipitation Maximum Time" displayString="Time of Maximum Precipitation" value="12Sep2013, 18:00" />
      <StatisticMeasure type="Precipitation Total" displayString="Precipitation Total" value="297.9999988" units="MM" />
      <StatisticMeasure type="Precipitation Volume" displayString="Precipitation Volume" value="14899.9999408" units="M3" />
      <StatisticMeasure type="Loss Maximum" displayString="Maximum Loss" value="5.5110418" units="MM" />
      <StatisticMeasure type="Loss Maximum Time" displayString="Time of Maximum Loss" value="12Sep2013, 17:00" />
      <StatisticMeasure type="Loss Total" displayString="Loss Total" value="257.9905942" units="MM" />
      <StatisticMeasure type="Loss Volume" displayString="Loss Volume" value="12899.5297117" units="M3" />
      <StatisticMeasure type="Excess Maximum" displayString="Maximum Excess" value="5.1285983" units="MM" />
      <StatisticMeasure type="Excess Maximum Time" displayString="Time of Maximum Excess" value="12Sep2013, 18:45" />
      <StatisticMeasure type="Excess Total" displayString="Excess Total" value="40.0094046" units="MM" />
      <StatisticMeasure type="Excess Volume" displayString="Excess Volume" value="2000.4702290" units="M3" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Baseflow" type="Source">
    <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Baseflow/FLOW//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Baseflow/FLOW-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="86040.0000000" units="M3" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="0.1000000" units="M3/S" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Junction-2" type="Junction">
    <ExecutionTime>31May2022, 19:25:32</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>Yes</IsComputationPoint>
    <DrainageArea area="" units="KM2" />
    <ObservedFlowGage name="Cheyenne Ck at Evans" />
    <FlowLink upstreamName="Reach-1" />
    <FlowLink upstreamName="Subbasin-3" />
    <FlowLink upstreamName="Baseflow" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Observed Flow" displayString="Observed Flow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW-OBSERVED//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Residual Flow" displayString="Residual Flow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW-RESIDUAL//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Observed Flow" displayString="Cumulative Observed Flow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW-OBSERVED-CUMULATIVE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Combined Inflow" displayString="Combined Inflow" />
        <DssFileName>Sep2013_AORC_Uncalib.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW-COMBINE//15MIN/RUN:Sep2013_AORC_Uncalib/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="28.5407598" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="3643774.9709674" units="M3" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="4.2311743" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="08Sep2013, 02:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="28.5407598" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="12Sep2013, 24:00" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="3643774.9709674" units="M3" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="4.2311743" units="M3/S" />
      <StatisticMeasure type="Observed Flow Minimum" displayString="Minimum Observed Flow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Observed Flow Minimum Time" displayString="Time of Minimum Observed Flow" value="09Sep2013, 09:00" />
      <StatisticMeasure type="Observed Flow Maximum" displayString="Maximum Observed Flow" value="41.5999985" units="M3/S" />
      <StatisticMeasure type="Observed Flow Maximum Time" displayString="Time of Maximum Observed Flow" value="12Sep2013, 23:30" />
      <StatisticMeasure type="Observed Flow Volume" displayString="Observed Flow Volume" value="4468094.9970905" units="M3" />
      <StatisticMeasure type="Observed Flow Average" displayString="Observed Flow Average" value="5.1902821" units="M3/S" />
      <StatisticMeasure type="Observed Flow RMSE Stdev" displayString="Observed Flow RMSE Stdev" value="0.5364471" units="M3/S" />
      <StatisticMeasure type="Observed Flow Nash Sutcliffe" displayString="Observed Flow Nash Sutcliffe" value="0.7122245" units="" />
      <StatisticMeasure type="Observed Flow Percent Bias" displayString="Observed Flow Percent Bias" value="-18.4789160" units="" />
      <StatisticMeasure type="Observed Flow Coefficient of Determination" displayString="Observed Flow Coefficient of Determination" value="0.7501084" units="" />
    </Statistics>
  </BasinElement>
</RunResults>

