{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["General","Precipitation","Channel","Chan. Chars.","Soils","Land Use","Input files","Output Files","Output Graphs"],"not_rendered":{"images":9,"macros":1,"external_links":1,"defined_names":80,"comments":22},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"General","index":0,"n_rows":11,"n_cols":18,"rows_kept":11,"flags":["formulas_cached_only"]}
[{"$nulls":17},true]
[null,"Simulation Control",{"$nulls":15},true]
[null,"          ",{"$nulls":15},true]
[null,"              ",{"$nulls":15},true]
[null,"Computational Time Step (DT): ",{"$nulls":3},5,"[sec]",{"$nulls":10},true]
[null,"Simulation Duration (SD):",{"$nulls":3},400,"minutes",{"$nulls":10},true]
[null,"Number of simulation iterations (NITER=SD/DT):",{"$nulls":3},{"v":4800,"d":"4800.0"},{"$nulls":11},true]
[null,"          ",{"$nulls":4},"          ",{"$nulls":10},true]
[{"$nulls":17},true]
[{"$nulls":17},false]
[{"$nulls":17},true]

{"sheet":"Precipitation","index":1,"n_rows":34,"n_cols":9,"rows_kept":34,"flags":["formulas_cached_only"]}
[]
[]
[null,"Precipitation Data",{"$nulls":3},"    ","    ","    ","    "]
[null,"   ","    ","    ","    ","    ","    ","    ","    "]
[null,"   ","    ","    ","    ","    ","    ","    ","    "]
[null,"   ","Precipitation duration: ",null,null,290,"[min]","    ","    "]
[null,"    ","For DT = ",5,"seconds, the number of rainfall intervals are: ",{"$nulls":3},{"v":3480,"d":"3480.0"}]
[null,"    ","    ","    ","    ","    ","    ","    ","    "]
[null,"    ","Uniform","    ","    ","    ","    ","    ","    "]
[null,"    ","    ","Intensity:",17,"[mm/hr]","    ","    ","    "]
[null,"    ","    ","    ","    ","    ","    ","    ","    "]
[null,"    ","Distributed",null,"    ","    ","    ","    ","    "]
[null,"    ","    ","Number of Raingages:",null,null,16,"    ","    "]
[null,"    ","    ","Rainfall Data Time Step (DR):",null,null,600,"[sec]","    "]
[null,"    ","    ","Ratio between rainfall time step and DT (DR/DT):",null,"    ","    ","    ",120]
[null,"    ","    ","    ","    ","    ","    ","    ","    "]
[null,"    ","    ","List of Used Raingages:",null,null,"    ","    ","    "]
[null,"    ","    ","Name",null,"X_Coordinate",null,"Y_Coordinate"]
[{"$nulls":3},1,null,231568.7117,null,3791553.7426]
[{"$nulls":3},2,null,233072.7721,null,3793603.9817]
[{"$nulls":3},5,null,236856.3335,null,3794839.5058]
[{"$nulls":3},6,null,236459.33,null,3795732.9309]
[{"$nulls":3},7,null,236662.9499,null,3793699.8824]
[{"$nulls":3},10,null,238396.5605,null,3794734.2989]
[{"$nulls":3},12,null,239756.4195,null,3795151.8743]
[{"$nulls":3},14,null,234644.3966,null,3793655.021]
[{"$nulls":3},34,null,237777.6768,null,3796476.9739]
[{"$nulls":3},35,null,238787.2374,null,3796056.2956]
[{"$nulls":3},41,null,233758.5726,null,3794401.0867]
[{"$nulls":3},42,null,235620.4058,null,3795906.558]
[{"$nulls":3},52,null,234840.6096,null,3792778.0814]
[{"$nulls":3},61,null,233122.6924,null,3791785.0733]
[{"$nulls":3},64,null,236523.6428,null,3792701.0902]
[{"$nulls":3},65,null,238663.3566,null,3793326.2882]

{"sheet":"Channel","index":2,"n_rows":35,"n_cols":9,"rows_kept":35,"flags":["formulas_cached_only"]}
[]
[null,"Basin Outlet Characteristics"]
[]
[]
[null,null,"Outlet channel cell: ",null,null,"Row:",35]
[{"$nulls":5},"Column: ",1]
[{"$nulls":5},"Overland Slope:",{"v":0.003368,"d":"0.00337"}]
[]
[null,null,"Explicit Channel Routing"]
[]
[]
[null,"Channel Links Characteristics",{"$nulls":6},"   "]
[null,"   ",{"$nulls":6},"   "]
[null,"   ",{"$nulls":6},"   "]
[null,"   ",{"$nulls":6},"   "]
[null,null,"Link","Total","Width","Depth","Manning n","Sinuosity","   "]
[null,null,"number","nodes","[m]","[m]",null,null,"   "]
[null,null,1,7,{"v":18,"d":"18.00"},{"v":3,"d":"3.00"},{"v":0.05,"d":"0.050"},1]
[null,null,2,8,{"v":22,"d":"22.00"},{"v":3.5,"d":"3.50"},{"v":0.05,"d":"0.050"},1]
[null,null,3,6,{"v":25,"d":"25.00"},{"v":4.3,"d":"4.30"},{"v":0.05,"d":"0.050"},1]
[null,null,4,5,{"v":28,"d":"28.00"},{"v":3.1,"d":"3.10"},{"v":0.05,"d":"0.050"},1]
[null,null,5,10,{"v":22.4,"d":"22.40"},{"v":4,"d":"4.00"},{"v":0.05,"d":"0.050"},1]
[null,null,6,11,{"v":29.4,"d":"29.40"},{"v":4.2,"d":"4.20"},{"v":0.05,"d":"0.050"},1]
[null,null,7,9,{"v":23,"d":"23.00"},4.35,{"v":0.05,"d":"0.050"},1]
[null,null,8,3,{"v":22,"d":"22.00"},{"v":4.1,"d":"4.10"},{"v":0.05,"d":"0.050"},1]
[null,null,9,12,{"v":30,"d":"30.00"},{"v":4.4,"d":"4.40"},{"v":0.05,"d":"0.050"},1]
[null,null,10,14,{"v":25,"d":"25.00"},{"v":4.3,"d":"4.30"},{"v":0.05,"d":"0.050"},1]
[null,null,11,11,{"v":30,"d":"30.00"},{"v":3.4,"d":"3.40"},{"v":0.05,"d":"0.050"},1]
[null,null,12,15,{"v":30,"d":"30.00"},3.55,{"v":0.05,"d":"0.050"},1]
[null,null,13,7,{"v":27,"d":"27.00"},{"v":4.5,"d":"4.50"},{"v":0.05,"d":"0.050"},1]
[null,null,14,8,{"v":30,"d":"30.00"},{"v":4.7,"d":"4.70"},{"v":0.05,"d":"0.050"},1]
[null,null,15,11,{"v":50,"d":"50.00"},{"v":5,"d":"5.00"},{"v":0.05,"d":"0.050"},1]
[null,null,16,8,{"v":25,"d":"25.00"},{"v":3.5,"d":"3.50"},{"v":0.05,"d":"0.050"},1]
[null,null,17,10,{"v":48,"d":"48.00"},{"v":5,"d":"5.00"},{"v":0.05,"d":"0.050"},1]
[null,null,18,11,{"v":34,"d":"34.00"},6.05,{"v":0.05,"d":"0.050"},1]

{"sheet":"Chan. Chars.","index":3,"n_rows":184,"n_cols":4,"rows_kept":184,"flags":["formulas_cached_only"]}
[1,7]
[18,3,0.05,1]
[18,3,0.05,1]
[18,3,0.05,1]
[18,3,0.05,1]
[18,3,0.05,1]
[18,3,0.05,1]
[18,3,0.05,1]
[2,8]
[22,3.5,0.05,1]
[22,3.5,0.05,1]
[22,3.5,0.05,1]
[22,3.5,0.05,1]
[22,3.5,0.05,1]
[22,3.5,0.05,1]
[22,3.5,0.05,1]
[22,3.5,0.05,1]
[3,6]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[4,5]
[28,3.1,0.05,1]
[28,3.1,0.05,1]
[28,3.1,0.05,1]
[28,3.1,0.05,1]
[28,3.1,0.05,1]
[5,10]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[22.4,4,0.05,1]
[6,11]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[29.4,4.2,0.05,1]
[7,9]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[23,4.35,0.05,1]
[8,3]
[22,4.1,0.05,1]
[22,4.1,0.05,1]
[22,4.1,0.05,1]
[9,12]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[30,4.4,0.05,1]
[10,14]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[25,4.3,0.05,1]
[11,11]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[30,3.4,0.05,1]
[12,15]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[30,3.55,0.05,1]
[13,7]
[27,4.5,0.05,1]
[27,4.5,0.05,1]
[27,4.5,0.05,1]
[27,4.5,0.05,1]
[27,4.5,0.05,1]
[27,4.5,0.05,1]
[27,4.5,0.05,1]
[14,8]
[30,4.7,0.05,1]
[30,4.7,0.05,1]
[30,4.7,0.05,1]
[30,4.7,0.05,1]
[30,4.7,0.05,1]
[30,4.7,0.05,1]
[30,4.7,0.05,1]
[30,4.7,0.05,1]
[15,11]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[50,5,0.05,1]
[16,8]
[25,3.5,0.05,1]
[25,3.5,0.05,1]
[25,3.5,0.05,1]
[25,3.5,0.05,1]
[25,3.5,0.05,1]
[25,3.5,0.05,1]
[25,3.5,0.05,1]
[25,3.5,0.05,1]
[17,10]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[48,5,0.05,1]
[18,11]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]
[34,6.05,0.05,1]

{"sheet":"Soils","index":4,"n_rows":22,"n_cols":10,"rows_kept":22,"flags":["formulas_cached_only"]}
[]
[]
[null,"Soil Parameters",null,null,"Number of different soil types:",null,7]
[null,"   ",null,null,"Infiltration",{"$nulls":3},"Erosion"]
[null,"Soil Type","Soil ","Hydr. Cond.","Suction Head","Moisture Deficit","Sand","Silt","Clay","KUSLE"]
[null,"    ","Index","[cm/h]","[cm]","[cm3/cm3]","[%]","[%]","[%]","[ -- ]"]
[null,"Calloway",1,{"v":0.35,"d":"0.350"},25,0.29,0.25,0.55,{"v":0.19999999999999996,"d":"0.20"},0.4]
[null,"Fallaya",2,{"v":0.35,"d":"0.350"},25,0.29,0.3,0.6,{"v":0.09999999999999998,"d":"0.10"},1]
[null,"Grenada",3,{"v":0.3,"d":"0.300"},20,0.29,0.25,0.55,{"v":0.19999999999999996,"d":"0.20"},0.4]
[null,"Loring",4,{"v":0.3,"d":"0.300"},25,0.29,0.25,0.55,{"v":0.19999999999999996,"d":"0.20"},0.4]
[null,"Collins",5,{"v":0.2,"d":"0.200"},20,0.29,0.3,0.6,{"v":0.09999999999999998,"d":"0.10"},0.3]
[null,"Memphis",6,{"v":0.35,"d":"0.350"},25,0.29,0.25,0.55,{"v":0.19999999999999996,"d":"0.20"},0.1]
[null,"Gullied Land",7,{"v":0.2,"d":"0.200"},15,0.29,0.25,0.55,{"v":0.19999999999999996,"d":"0.20"},0.1]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]
[null,null,"",{"$nulls":5},""]

{"sheet":"Land Use","index":5,"n_rows":22,"n_cols":7,"rows_kept":22,"flags":["formulas_cached_only"]}
[]
[]
[null,"Land Use Parameters"]
[null,"Number of different land use classes:",{"$nulls":4},4]
[null,"Land Use Type","Land Use","Manning n","Interception","CUSLE","PUSLE"]
[null,null,"Index","[--]","[mm]","[--]","[--]"]
[null,"Forest",1,0.25,3,0.07,1]
[null,"Water",2,0.01,0,0,1]
[null,"Cultivated",3,0.15,1,0.65,1]
[null,"Pasture",4,0.2,1.5,0.7,1]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]
[null,null,""]

{"sheet":"Input files","index":6,"n_rows":19,"n_cols":8,"rows_kept":19,"flags":["formulas_cached_only"]}
[]
[null,"Input Files"]
[]
[{"$nulls":4},"Name"]
[null,null,"Simulation control",null,"Input/control.dat"]
[null,null,"Precipitation [in/hr]",null,"Input/10minAver.pre"]
[null,null,"Channel",null,"input/chann0.05.dat"]
[]
[]
[null,null,"ArcInfo ASCII Input Grids",{"$nulls":4},"in meters"]
[{"$nulls":7},"in feet"]
[{"$nulls":4},"Name"]
[null,null,"Elevation ","in meters","Input/DEM150mod.asc"]
[null,null,"Soil",null,"Input/soils150mod.asc"]
[null,null,"Landuse",null,"Input/luse150mod.asc"]
[null,null,"Shape",null,"Input/mask.asc"]
[null,null,"Link",null,"Input/links.asc"]
[null,null,"Node",null,"Input/nodes.asc"]
[null,null,"Storage_Depth [m]"]

{"sheet":"Output Files","index":7,"n_rows":32,"n_cols":5,"rows_kept":32,"merged":[[3,3,3,5],[4,3,4,5],[5,3,5,5],[6,3,6,5],[14,3,14,5],[15,3,15,5],[16,3,16,5],[17,3,17,5],[18,3,18,5],[19,3,19,5],[20,3,20,5],[21,3,21,5],[22,3,22,5],[23,3,23,5],[24,3,24,5],[25,3,25,5],[26,3,26,5],[27,3,27,5],[28,3,28,5]],"flags":["formulas_cached_only"]}
[]
[null,"Output Files"]
[]
[{"$nulls":3},"Name"]
[null,null,"Summary file:","Output/run1.sum"]
[null,null,"Discharge [m3/s]:","Output/run1.q"]
[null,null,"Sediment discharge [m3/s]:","Output/run1.qs"]
[]
[null,null,"Write discharge (WD) and sediment discharge every",1,"minutes"]
[null,null,"Number of time steps to write the output (WD/DT):",12]
[]
[]
[null,"Time Series Output Grids"]
[]
[{"$nulls":3},"Name"]
[null,null,"Rainfall rates [mm/hr]","OutMaps/rain"]
[null,null,"Volume of infiltrated water [mm]","OutMaps/infvol"]
[null,null,"Water depth (channels and overland)[m]","OutMaps/depth"]
[null,null,"Volume of suspended sediment [mm]","OutMaps/SusSed"]
[null,null,"Sediment concentration  [m3/m3]","OutMaps/SedC"]
[null,null,"Net sediment volume [mm]","OutMaps/ErosDep"]
[null,null,"Total sand flux out [m3/s]","OutMaps/SandFlux"]
[null,null,"Total silt flux out [m3/s]","OutMaps/SiltFlux"]
[null,null,"Total clay flux out [m3/s]","OutMaps/ClayFlux"]
[null,null,"Total sediment flux out [m3/s]","OutMaps/SedFlux"]
[null,null,"Max. flux-averaged concentration of sand","OutMaps/sandMFAC"]
[null,null,"Max. flux-averaged concentration of silt ","OutMaps/siltMFAC"]
[null,null,"Max. flux-averaged concentration of clay","OutMaps/clayMFAC"]
[null,null,"Total max. flux-averaged concentration","OutMaps/sedMFAC"]
[]
[null,null,"Update graphic (UG) display every ",100,"minutes"]
[null,null,"Number of time steps to update graphics (UG/DT):",1200]

{"sheet":"Output Graphs","index":8,"n_rows":30,"n_cols":11,"rows_kept":30,"flags":["formulas_cached_only"]}
[]
[null,"Output Hydrographs/Sedigraphs"]
[]
[null,null,"Write discharge at internal locations."]
[null,null,"Number of internal locations:",6,{"$nulls":6},"m3/s"]
[null,null,"Hydrograph units:","mm/h",null,"Drainage",{"$nulls":4},"cfs"]
[null,null,"Location","Row","Column","area [ha]",{"$nulls":4},"mm/h"]
[null,null,"Outlet (231568.712; 3791553.743)",35,1,2052]
[null,null,"Station 4 (235367.347 ;3794280.517)",17,26,344.25]
[null,null,"Station 6 (236459.330; 3795732.931)",7,33,137.25]
[null,null,"Station 7 (236662.950; 3793699.882)",20,34,171]
[null,null,"Station 8 (238577.958; 3795483.805)",8,47,148.5]
[null,null,"Station 14 (234644.397; 3793655.021)",21,22,139.5]
{"$rows_empty":7}
[null,null,"Write sediment discharge at internal locations."]
[null,null,"Number of internal locations:",6,{"$nulls":6},"m3/s"]
[null,null,"Sedigraph units:","tons/ha/day",null,"Drainage",{"$nulls":4},"tons/ha/day"]
[null,null,"Location","Row","Column","area [ha]"]
[null,null,"Outlet (231568.712; 3791553.743)",35,1,2052]
[null,null,"Station 4 (235367.347 ;3794280.517)",17,26,344.25]
[null,null,"Station 6 (236459.330; 3795732.931)",7,33,137.25]
[null,null,"Station 7 (236662.950; 3793699.882)",20,34,171]
[null,null,"Station 8 (238577.958; 3795483.805)",8,47,148.5]
[null,null,"Station 14 (234644.397; 3793655.021)",21,22,139.5]