<?xml version="1.0" encoding="UTF-8"?>
<RunResults>
  <RunName>Comb_HMS_6-hr 10^6-yr</RunName>
  <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
  <StartTime>31Dec1999, 24:00</StartTime>
  <EndTime>08Jan2000, 24:00</EndTime>
  <BasinElement name="Subbasin-1" type="Subbasin">
    <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
    <SubbasinArea area="29.77" units="KM2" />
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="29.77" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-CUMULATIVE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Incremental Precip" displayString="Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-INC//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Precip" displayString="Cumulative Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Excess" displayString="Canopy Overflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/EXCESS-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Potential ET" displayString="Potential Evapotranspiration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-POTENTIAL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy ET" displayString="Canopy Evapotranspiration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/ET-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Storage" displayString="Canopy Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/STORAGE-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Infiltration" displayString="Soil Infiltration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/INFILTRATION//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Storage" displayString="Soil Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/STORAGE-SOIL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Percolation" displayString="Soil Percolation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PERC-SOIL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Saturation Fraction" displayString="Saturation Fraction" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/SATURATION FRACTION//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Storage" displayString="Groundwater 1 Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/STORAGE-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Release" displayString="Groundwater 1 Lateral Flow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/OUTFLOW-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Percolation" displayString="Groundwater 1 Percolation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PERC-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Excess" displayString="Excess Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-EXCESS//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Excess" displayString="Cumulative Excess Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-EXCESS-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Loss" displayString="Precipitation Loss" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-LOSS//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Loss" displayString="Cumulative Precipitation Loss" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/PRECIP-LOSS-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Direct Runoff" displayString="Direct Runoff" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-DIRECT//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Baseflow" displayString="Baseflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/FLOW-BASE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Aquifer Recharge" displayString="Aquifer Recharge" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-1/AQUIFER RECHARGE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="0.0000000" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="0.0000000" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="41.4084141" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="1711249.7988391" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="57.4823580" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="2.4725476" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum" displayString="Minimum Direct Flow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum Time" displayString="Time of Minimum Direct Flow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Direct Flow Maximum" displayString="Maximum Direct Flow" value="40.9718396" units="M3/S" />
      <StatisticMeasure type="Direct Flow Maximum Time" displayString="Time of Maximum Direct Flow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Direct Flow Volume" displayString="Direct Flow Volume" value="1305135.9719060" units="M3" />
      <StatisticMeasure type="Direct Flow Depth" displayString="Direct Flow Depth" value="43.8406440" units="MM" />
      <StatisticMeasure type="Direct Flow Average" displayString="Direct Flow Average" value="1.8857621" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum" displayString="Minimum Baseflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum Time" displayString="Time of Minimum Baseflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Baseflow Maximum" displayString="Maximum Baseflow" value="3.0402682" units="M3/S" />
      <StatisticMeasure type="Baseflow Maximum Time" displayString="Time of Maximum Baseflow" value="01Jan2000, 23:15" />
      <StatisticMeasure type="Baseflow Volume" displayString="Baseflow Volume" value="406113.8269331" units="M3" />
      <StatisticMeasure type="Baseflow Depth" displayString="Baseflow Depth" value="13.6417140" units="MM" />
      <StatisticMeasure type="Baseflow Average" displayString="Baseflow Average" value="0.5867854" units="M3/S" />
      <StatisticMeasure type="Precipitation Maximum" displayString="Maximum Precipitation" value="24.2500000" units="MM" />
      <StatisticMeasure type="Precipitation Maximum Time" displayString="Time of Maximum Precipitation" value="01Jan2000, 01:15" />
      <StatisticMeasure type="Precipitation Total" displayString="Precipitation Total" value="152.4299998" units="MM" />
      <StatisticMeasure type="Precipitation Volume" displayString="Precipitation Volume" value="4537841.0948896" units="M3" />
      <StatisticMeasure type="Loss Maximum" displayString="Maximum Loss" value="10.1185418" units="MM" />
      <StatisticMeasure type="Loss Maximum Time" displayString="Time of Maximum Loss" value="01Jan2000, 01:00" />
      <StatisticMeasure type="Loss Total" displayString="Loss Total" value="108.5893558" units="MM" />
      <StatisticMeasure type="Loss Volume" displayString="Loss Volume" value="3232705.1229836" units="M3" />
      <StatisticMeasure type="Excess Maximum" displayString="Maximum Excess" value="15.3930925" units="MM" />
      <StatisticMeasure type="Excess Maximum Time" displayString="Time of Maximum Excess" value="01Jan2000, 01:15" />
      <StatisticMeasure type="Excess Total" displayString="Excess Total" value="43.8406440" units="MM" />
      <StatisticMeasure type="Excess Volume" displayString="Excess Volume" value="1305135.9719060" units="M3" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Subbasin-2" type="Subbasin">
    <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
    <SubbasinArea area="26.54" units="KM2" />
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="26.54" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW-CUMULATIVE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Incremental Precip" displayString="Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-INC//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Precip" displayString="Cumulative Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Excess" displayString="Canopy Overflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/EXCESS-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Potential ET" displayString="Potential Evapotranspiration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/ET-POTENTIAL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy ET" displayString="Canopy Evapotranspiration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/ET-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Storage" displayString="Canopy Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/STORAGE-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Infiltration" displayString="Soil Infiltration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/INFILTRATION//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Storage" displayString="Soil Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/STORAGE-SOIL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Percolation" displayString="Soil Percolation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PERC-SOIL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Saturation Fraction" displayString="Saturation Fraction" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/SATURATION FRACTION//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Storage" displayString="Groundwater 1 Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/STORAGE-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Release" displayString="Groundwater 1 Lateral Flow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/OUTFLOW-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Percolation" displayString="Groundwater 1 Percolation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PERC-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Excess" displayString="Excess Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-EXCESS//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Excess" displayString="Cumulative Excess Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-EXCESS-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Loss" displayString="Precipitation Loss" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-LOSS//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Loss" displayString="Cumulative Precipitation Loss" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/PRECIP-LOSS-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Direct Runoff" displayString="Direct Runoff" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW-DIRECT//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Baseflow" displayString="Baseflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/FLOW-BASE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Aquifer Recharge" displayString="Aquifer Recharge" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-2/AQUIFER RECHARGE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="0.0000000" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="0.0000000" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="45.5017249" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="1732277.6277584" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="65.2704457" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="2.5029300" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum" displayString="Minimum Direct Flow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum Time" displayString="Time of Minimum Direct Flow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Direct Flow Maximum" displayString="Maximum Direct Flow" value="45.1585456" units="M3/S" />
      <StatisticMeasure type="Direct Flow Maximum Time" displayString="Time of Maximum Direct Flow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Direct Flow Volume" displayString="Direct Flow Volume" value="1428651.6680199" units="M3" />
      <StatisticMeasure type="Direct Flow Depth" displayString="Direct Flow Depth" value="53.8301307" units="MM" />
      <StatisticMeasure type="Direct Flow Average" displayString="Direct Flow Average" value="2.0642272" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum" displayString="Minimum Baseflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum Time" displayString="Time of Minimum Baseflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Baseflow Maximum" displayString="Maximum Baseflow" value="2.3809301" units="M3/S" />
      <StatisticMeasure type="Baseflow Maximum Time" displayString="Time of Maximum Baseflow" value="01Jan2000, 21:00" />
      <StatisticMeasure type="Baseflow Volume" displayString="Baseflow Volume" value="303625.9597385" units="M3" />
      <StatisticMeasure type="Baseflow Depth" displayString="Baseflow Depth" value="11.4403150" units="MM" />
      <StatisticMeasure type="Baseflow Average" displayString="Baseflow Average" value="0.4387028" units="M3/S" />
      <StatisticMeasure type="Precipitation Maximum" displayString="Maximum Precipitation" value="24.2500000" units="MM" />
      <StatisticMeasure type="Precipitation Maximum Time" displayString="Time of Maximum Precipitation" value="01Jan2000, 01:15" />
      <StatisticMeasure type="Precipitation Total" displayString="Precipitation Total" value="152.4299998" units="MM" />
      <StatisticMeasure type="Precipitation Volume" displayString="Precipitation Volume" value="4045492.1954441" units="M3" />
      <StatisticMeasure type="Loss Maximum" displayString="Maximum Loss" value="8.7505415" units="MM" />
      <StatisticMeasure type="Loss Maximum Time" displayString="Time of Maximum Loss" value="01Jan2000, 00:45" />
      <StatisticMeasure type="Loss Total" displayString="Loss Total" value="98.5998692" units="MM" />
      <StatisticMeasure type="Loss Volume" displayString="Loss Volume" value="2616840.5274242" units="M3" />
      <StatisticMeasure type="Excess Maximum" displayString="Maximum Excess" value="17.1053379" units="MM" />
      <StatisticMeasure type="Excess Maximum Time" displayString="Time of Maximum Excess" value="01Jan2000, 01:15" />
      <StatisticMeasure type="Excess Total" displayString="Excess Total" value="53.8301307" units="MM" />
      <StatisticMeasure type="Excess Volume" displayString="Excess Volume" value="1428651.6680199" units="M3" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Junction-1" type="Junction">
    <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="56.31" units="KM2" />
    <FlowLink upstreamName="Subbasin-1" />
    <FlowLink upstreamName="Subbasin-2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-CUMULATIVE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Combined Inflow" displayString="Combined Inflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Junction-1/FLOW-COMBINE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="86.9101390" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="3443527.4265975" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="61.1530355" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="4.9754776" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="86.9101390" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="3443527.4265975" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="61.1530355" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="4.9754776" units="M3/S" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Reach-1" type="Reach">
    <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="56.31" units="KM2" />
    <FlowLink upstreamName="Junction-1" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW-CUMULATIVE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Combined Inflow" displayString="Combined Inflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW-COMBINE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Flow Velocity" displayString="Flow Velocity" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Reach-1/FLOW-VELOCITY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="86.9101390" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="3443527.4265975" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="61.1530355" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="4.9754776" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="86.8946422" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="3443625.6278898" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="61.1547794" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="4.9756195" units="M3/S" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Subbasin-3" type="Subbasin">
    <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
    <SubbasinArea area="0.05" units="KM2" />
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="0.05" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW-CUMULATIVE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Incremental Precip" displayString="Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-INC//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Precip" displayString="Cumulative Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Excess" displayString="Canopy Overflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/EXCESS-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Potential ET" displayString="Potential Evapotranspiration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/ET-POTENTIAL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy ET" displayString="Canopy Evapotranspiration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/ET-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Canopy Storage" displayString="Canopy Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/STORAGE-CANOPY//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Infiltration" displayString="Soil Infiltration" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/INFILTRATION//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Storage" displayString="Soil Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/STORAGE-SOIL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Percolation" displayString="Soil Percolation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PERC-SOIL//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Soil Saturation Fraction" displayString="Saturation Fraction" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/SATURATION FRACTION//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Storage" displayString="Groundwater 1 Storage" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/STORAGE-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Release" displayString="Groundwater 1 Lateral Flow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/OUTFLOW-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="GW1 Percolation" displayString="Groundwater 1 Percolation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PERC-GW-1//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Excess" displayString="Excess Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-EXCESS//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Excess" displayString="Cumulative Excess Precipitation" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-EXCESS-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Precip Loss" displayString="Precipitation Loss" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-LOSS//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Loss" displayString="Cumulative Precipitation Loss" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/PRECIP-LOSS-CUM//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Direct Runoff" displayString="Direct Runoff" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW-DIRECT//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Baseflow" displayString="Baseflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/FLOW-BASE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Aquifer Recharge" displayString="Aquifer Recharge" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Subbasin-3/AQUIFER RECHARGE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="0.0000000" units="M3" />
      <StatisticMeasure type="Inflow Depth" displayString="Inflow Depth" value="0.0000000" units="MM" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="0.0823711" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Jan2000, 03:00" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="3097.2180226" units="M3" />
      <StatisticMeasure type="Outflow Depth" displayString="Outflow Depth" value="61.9443605" units="MM" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="0.0044751" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum" displayString="Minimum Direct Flow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Direct Flow Minimum Time" displayString="Time of Minimum Direct Flow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Direct Flow Maximum" displayString="Maximum Direct Flow" value="0.0822828" units="M3/S" />
      <StatisticMeasure type="Direct Flow Maximum Time" displayString="Time of Maximum Direct Flow" value="01Jan2000, 03:00" />
      <StatisticMeasure type="Direct Flow Volume" displayString="Direct Flow Volume" value="2529.7925496" units="M3" />
      <StatisticMeasure type="Direct Flow Depth" displayString="Direct Flow Depth" value="50.5958510" units="MM" />
      <StatisticMeasure type="Direct Flow Average" displayString="Direct Flow Average" value="0.0036552" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum" displayString="Minimum Baseflow" value="0.0000000" units="M3/S" />
      <StatisticMeasure type="Baseflow Minimum Time" displayString="Time of Minimum Baseflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Baseflow Maximum" displayString="Maximum Baseflow" value="0.0045495" units="M3/S" />
      <StatisticMeasure type="Baseflow Maximum Time" displayString="Time of Maximum Baseflow" value="01Jan2000, 18:00" />
      <StatisticMeasure type="Baseflow Volume" displayString="Baseflow Volume" value="567.4254730" units="M3" />
      <StatisticMeasure type="Baseflow Depth" displayString="Baseflow Depth" value="11.3485095" units="MM" />
      <StatisticMeasure type="Baseflow Average" displayString="Baseflow Average" value="0.0008199" units="M3/S" />
      <StatisticMeasure type="Precipitation Maximum" displayString="Maximum Precipitation" value="24.2500000" units="MM" />
      <StatisticMeasure type="Precipitation Maximum Time" displayString="Time of Maximum Precipitation" value="01Jan2000, 01:15" />
      <StatisticMeasure type="Precipitation Total" displayString="Precipitation Total" value="152.4299998" units="MM" />
      <StatisticMeasure type="Precipitation Volume" displayString="Precipitation Volume" value="7621.4999914" units="M3" />
      <StatisticMeasure type="Loss Maximum" displayString="Maximum Loss" value="8.6183189" units="MM" />
      <StatisticMeasure type="Loss Maximum Time" displayString="Time of Maximum Loss" value="01Jan2000, 00:45" />
      <StatisticMeasure type="Loss Total" displayString="Loss Total" value="101.8341488" units="MM" />
      <StatisticMeasure type="Loss Volume" displayString="Loss Volume" value="5091.7074418" units="M3" />
      <StatisticMeasure type="Excess Maximum" displayString="Maximum Excess" value="16.7204363" units="MM" />
      <StatisticMeasure type="Excess Maximum Time" displayString="Time of Maximum Excess" value="01Jan2000, 01:15" />
      <StatisticMeasure type="Excess Total" displayString="Excess Total" value="50.5958510" units="MM" />
      <StatisticMeasure type="Excess Volume" displayString="Excess Volume" value="2529.7925496" units="M3" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Baseflow" type="Source">
    <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>No</IsComputationPoint>
    <DrainageArea area="" units="KM2" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Baseflow/FLOW//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Baseflow/FLOW-CUMULATIVE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="69120.0000000" units="M3" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="0.1000000" units="M3/S" />
    </Statistics>
  </BasinElement>
  <BasinElement name="Junction-2" type="Junction">
    <ExecutionTime>24Jun2021, 16:24:15</ExecutionTime>
    <UnitSystem>SI</UnitSystem>
    <IsComputationPoint>Yes</IsComputationPoint>
    <DrainageArea area="" units="KM2" />
    <ObservedFlowGage name="Cheyenne Ck at Evans" />
    <FlowLink upstreamName="Reach-1" />
    <FlowLink upstreamName="Subbasin-3" />
    <FlowLink upstreamName="Baseflow" />
    <Hydrology>
      <TimeSeries>
        <TimeSeriesType type="Outflow" displayString="Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Cumulative Outflow" displayString="Cumulative Outflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW-CUMULATIVE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
      <TimeSeries>
        <TimeSeriesType type="Combined Inflow" displayString="Combined Inflow" />
        <DssFileName>Comb_HMS_6_hr_10_6_yr.dss</DssFileName>
        <DssPathname>//Junction-2/FLOW-COMBINE//15MIN/RUN:Comb_HMS_6-hr 10^6-yr/</DssPathname>
      </TimeSeries>
    </Hydrology>
    <Sediment />
    <WaterQuality />
    <Statistics>
      <StatisticMeasure type="Inflow Minimum" displayString="Minimum Inflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Inflow Minimum Time" displayString="Time of Minimum Inflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Inflow Maximum" displayString="Maximum Inflow" value="87.0709181" units="M3/S" />
      <StatisticMeasure type="Inflow Maximum Time" displayString="Time of Maximum Inflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Inflow Volume" displayString="Inflow Volume" value="3515842.8459123" units="M3" />
      <StatisticMeasure type="Inflow Average" displayString="Inflow Average" value="5.0800946" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum" displayString="Minimum Outflow" value="0.1000000" units="M3/S" />
      <StatisticMeasure type="Outflow Minimum Time" displayString="Time of Minimum Outflow" value="31Dec1999, 24:00" />
      <StatisticMeasure type="Outflow Maximum" displayString="Maximum Outflow" value="87.0709181" units="M3/S" />
      <StatisticMeasure type="Outflow Maximum Time" displayString="Time of Maximum Outflow" value="01Jan2000, 03:45" />
      <StatisticMeasure type="Outflow Volume" displayString="Outflow Volume" value="3515842.8459123" units="M3" />
      <StatisticMeasure type="Outflow Average" displayString="Outflow Average" value="5.0800946" units="M3/S" />
    </Statistics>
  </BasinElement>
</RunResults>

